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MATERIAL SAFETY DATA SHEET
ETHYLENE GLYCOL DIMETHYL ETHER 99%
(Extra Pure)
(Monoglyme)
MSDS CAS: 110-71-4
	Section 1: Chemical Product and Company Identification



Section 1: Chemical Product 
Product Name: ETHYLENE GLYCOL DIMETHYL ETHER
CAS#:110-71-4
Synonym:1,2-Dimethoxyethane, Monoglyme
Chemical Name: Ethylene Glycol Dimethyl Ether
Chemical Formula:C4H10O2


Brand: OXFORD
Details Of The Supplier Of The Safety Data Sheet :
Company identification:   OXFORD LAB FINE CHEM LLP
				Unit. No. 12, 1st Floor, Neminath Industrial Estate No. 6,
Navghar, Vasai (East). Palghar - 401 210.
				Mumbai, Maharashtra, INDIA.
				       Tel: 91-250-2390989	
				       Tel/Fax:  91-250-2390032

	Section 2: Composition and Information on Ingredients



Composition:
	Name
	CAS #
	% by Weight

	Ethylene Glycol Dimethyl Ether
	110-71-4
	99%



Toxicological Data on Ingredients:Ethylene Glycol Dimethyl Ether LD50: Not available. LC50: Not available.

	Section 3: Hazards Identification



Potential Acute Health Effects:
Very hazardous in case of ingestion. Hazardous in case of skin contact (irritant), of eye contact (irritant), of inhalation. Slightly hazardous in case of skin contact (permeator).

Potential Chronic Health Effects:
CARCINOGENIC EFFECTS: Not available. MUTAGENIC EFFECTS: Not available. TERATOGENIC EFFECTS: Not available. DEVELOPMENTAL TOXICITY: Not available. The substance is toxic to lungs, mucous membranes. Repeated or prolonged exposure to the substance can produce target organs damage.

	Section 4: First Aid Measures



Eye Contact:
Check for and remove any contact lenses. Immediately flush eyes with running water for at least 15 minutes, keeping eyelids open. Cold water may be used. Do not use an eye ointment. Seek medical attention.

Skin Contact:
After contact with skin, wash immediately with plenty of water. Gently and thoroughly wash the contaminated skin with running water and non-abrasive soap. Be particularly careful to clean folds, crevices, creases and groin. Cold water may be used. Cover the irritated skin with an emollient. If irritation persists, seek medical attention. Wash contaminated clothing before reusing.

Serious Skin Contact:
Wash with a disinfectant soap and cover the contaminated skin with an anti-bacterial cream. Seek medical attention.

Inhalation:Allow the victim to rest in a well ventilated area. Seek immediate medical attention.

Serious Inhalation:
Evacuate the victim to a safe area as soon as possible. Loosen tight clothing such as a collar, tie, belt or waistband. If breathing is difficult, administer oxygen. If the victim is not breathing, perform mouth-to-mouth resuscitation. Seek medical attention.

Ingestion:
Do not induce vomiting. Loosen tight clothing such as a collar, tie, belt or waistband. If the victim is not breathing, perform mouth-to-mouth resuscitation. Seek immediate medical attention.

Serious Ingestion:Not available.

	Section 5: Fire and Explosion Data



Flammability of the Product:Flammable.

Auto-Ignition Temperature:202°C (395.6°F)

Flash Points:CLOSED CUP: 4.5°C (40.1°F).

Flammable Limits:LOWER: 1.6%

Products of Combustion:These products are carbon oxides (CO, CO2).

Fire Hazards in Presence of Various Substances:Flammable in presence of open flames and sparks.

Explosion Hazards in Presence of Various Substances:
Risks of explosion of the product in presence of mechanical impact: Not available. Risks of explosion of the product in presence of static discharge: Not available.

Fire Fighting Media and Instructions:
Flammable liquid, soluble or dispersed in water. 
SMALL FIRE: Use DRY chemical powder. 
LARGE FIRE: Use alcohol foam, water spray or fog.

Special Remarks on Fire Hazards:Not available.

Special Remarks on Explosion Hazards:Not available.

	Section 6: Accidental Release Measures




Small Spill:
Dilute with water and mop up, or absorb with an inert dry material and place in an appropriate waste disposal container.

Large Spill:
Flammable liquid. Keep away from heat. Keep away from sources of ignition. Stop leak if without risk. Absorb with DRY earth, sand or other non-combustible material. Do not touch spilled material. Prevent entry into sewers, basements or confined areas; dike if needed. Eliminate all ignition sources.

	Section 7: Handling and Storage



Precautions:
Keep away from heat. Keep away from sources of ignition. Ground all equipment containing material. Do not breathe gas/ fumes/ vapour/spray. Wear suitable protective clothing In case of insufficient ventilation, wear suitable respiratory equipment if you feel unwell, seek medical attention and show the label when possible. Avoid contact with skin and eyes.

Storage:
Flammable materials should be stored in a separate safety storage cabinet or room. Keep away from heat. Keep away from sources of ignition. Keep container tightly closed. Keep in a cool, well-ventilated place. Ground all equipment containing material. A refrigerated room would be preferable for materials with a flash point lower than 37.8°C (100°F).

	Section 8: Exposure Controls/Personal Protection



Engineering Controls:
Provide exhaust ventilation or other engineering controls to keep the airborne concentrations of vapors below their respective threshold limit value. Ensure that eyewash stations and safety showers are proximal to the work-station location.

Personal Protection:
Splash goggles. Lab coat. Vapor respirator. Be sure to use an approved/certified respirator or equivalent. Gloves.

Personal Protection in Case of a Large Spill:
Splash goggles. Full suit. Vapor respirator. Boots. Gloves. A self contained breathing apparatus should be used to avoid inhalation of the product. Suggested protective clothing might not be sufficient; consult a specialist BEFORE handling this product.

Exposure Limits:Not available.

	Section 9: Physical and Chemical Properties


Physical state and appearance	: Liquid.
Odor						: Not available.
Taste						: Not available.
Molecular Weight			: 90.12 g/mole
Color						: Not available.
	Section 9: Physical and Chemical Properties (Continued)




pH (1% soln/water)		: Not available.
Boiling Point			: 83.5°C (182.3°F)
Melting Point			: -58°C (-72.4°F)
Critical Temperature		: Not available.
Specific Gravity			: 0.863 (Water = 1)
Vapor Pressure			: 48 mm of Hg (@ 20°C)
Vapor Density			: 3.11 (Air = 1)
Volatility				: Not available.
Odor Threshold			: Not available.
Water/Oil Dist. Coeff.		: Not available.
Ionicity (in Water)		: Not available.
Dispersion Properties		: See solubility in water.
Solubility				: Easily soluble in cold water.


	Section 10: Stability and Reactivity Data




Stability:The product is stable.

Instability Temperature:Not available.

Conditions of Instability:Not available.

Incompatibility with various substances:Not available.

Corrosivity:Non-corrosive in presence of glass.

Special Remarks on Reactivity:Not available.

Special Remarks on Corrosivity:Not available.

Polymerization:No.



	Section 11: Toxicological Information



Routes of Entry:Eye contact. Inhalation. Ingestion.

Toxicity to Animals:LD50: Not available. LC50: Not available.

Chronic Effects on Humans:The substance is toxic to lungs, mucous membranes.

Other Toxic Effects on Humans:
Very hazardous in case of ingestion. Hazardous in case of skin contact (irritant), of inhalation. Slightly hazardous in case of skin contact (permeator).

Special Remarks on Toxicity to Animals:Not available.

Special Remarks on Chronic Effects on Humans:Not available.

Special Remarks on other Toxic Effects on Humans:Not available.


	Section 12: Ecological Information


Ecotoxicity:Not available.

BOD5 and COD:Not available.

Products of Biodegradation:
Possibly hazardous short term degradation products are not likely. However, long term degradation products may arise.

Toxicity of the Products of Biodegradation:The products of degradation are more toxic.

Special Remarks on the Products of Biodegradation:Not available.

	Section 13: Disposal Considerations




Waste Disposal:
	Section 14: Transport Information



Land transport (ADR-RID)

Proper shipping name    : 1,2-DIMETHOXYETHANE
UN N°                               : 2252
H.I. nr                              : 33
ADR – Class                    : 3
Labelling – Transport    : 3 : Flammable liquid.
ADR – Group                  : II


Sea transport (IMDG) [English only]

Proper shipping name   : 1,2-DIMETHOXYETHANE
UN N°                              : 2252
IMO-IMDG - Class or division  : 3 : Flammable liquid.
IMO-IMDG - Packing group  : II

Air transport (ICAO-IATA) [English only]

Proper shipping name   : 1,2-DIMETHOXYETHANE
UN N°                              : 2252
IATA - Class or division : 3 : Flammable liquid.
IATA - Packing group    : II

	Section 15: Other Regulatory Information



Federal and State Regulations:Pennsylvania RTK: Ethylene Glycol Dimethyl EtherMassachusetts RTK: Ethylene Glycol Dimethyl EtherTSCA 8(b) inventory: Ethylene Glycol Dimethyl Ether

Other Regulations: 
OSHA: Hazardous by definition of Hazard Communication Standard (29 CFR 1910.1200).

Other Classifications:
WHMIS (Canada): CLASS B-2: Flammable liquid with a flash point lower than 37.8°C (100°F). CLASS D-2A: Material causing other toxic effects(VERY TOXIC).
DSCL (EEC): R11- Highly flammable. R36/38- Irritating to eyes and skin.
	Section 15: Other Regulatory Information (Continued)




HMIS (U.S.A.):
Health Hazard: 2
Fire Hazard: 3
Reactivity: 0
Personal Protection: h

National Fire Protection Association (U.S.A.):
Health: 2
Flammability: 2
Reactivity: 0
Specific hazard:

Protective Equipment:
Gloves. Lab coat. Vapor respirator. Be sure to use an approved/certified respirator or equivalent. Wear appropriate respirator when ventilation is inadequate. Splash goggles.


	Section 16 - Additional Information



References: Not available.
Other Special Considerations: Not available.






Disclaimer:
**************************************************************************************************************************
The information contained herein in good faith but makes no representations as to its comprehensiveness or accuracy. This document is intended only as a guide to the appropriate precautionary handling of the material by a properly trained person using this product. Individuals receiving the information must exercise their independent judgment in determining its appropriateness for a particular purpose.	
Oxford Lab Fine ChemLLP makes no representations or warranties, either express or implied, including without limitation any warranties of merchantability, fitness for a particular purpose with respect to the information set forth herein or the product to which the information refers. Accordingly, Oxford Lab Fine Chem LLP will not be responsible for damages resulting from use of or reliance upon this information.
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